
B2 (ex B7) Gleeble samples:

Heating at 5C/s up to 1000C, then cooling down to room temperature at the following rates:
enfriamiento a: 0.2, 0.5 y 1 C/seg.

Gleeble file     Cooling rate
SteelB1.D12      5°C/s
SteelB1.D13      2°C/s
SteelB1.D14      1.5°C/s
SteelB1.D15      1°C/s
SteelB1.D16      0.75°C/s
SteelB1.D17      0.5°C/s
SteelB1.D18      0.1°C/s
SteelB1.D19      0.2°C/s

Heating at 5C/s up to 880C, 5 minutes of holding, then cooling down to room temperature at the following rates:

Gleeble file     Cooling rate
SteelB1.D20      0.2 °C/s
SteelB1.D21      0.5 °C/s
SteelB1.D22      1   °C/s

It is important to notice that Gleeble dilatometric files are named SteelB1.dX, but from d12 and onwards they correspond to B2 (ex B7) samples.

In Gleeble files Ptemp is the programmed temperature and TC1 is the measured one.
