
B2 (ex B7) Gleeble samples:

Heating at 5C/s up to 1000C, then cooling down to room temperature at the following rates:
enfriamiento a: 0.2, 0.5 y 1 C/seg.

Gleeble file     Cooling rate
SteelB1.D12      5°C/s
SteelB1.D13      2°C/s
SteelB1.D14      1.5°C/s
SteelB1.D15      1°C/s
SteelB1.D16      0.75°C/s
SteelB1.D17      0.5°C/s
SteelB1.D18      0.1°C/s
SteelB1.D19      0.2°C/s

Heating at 5C/s up to 880C, 5 minutes of holding, then cooling down to room temperature at the following rates:

Gleeble file     Cooling rate
SteelB1.D20      0.2 °C/s
SteelB1.D21      0.5 °C/s
SteelB1.D22      1   °C/s

It is important to notice that Gleeble dilatometric files are named SteelB1.dX, but from d12 and onwards they correspond to B2 (ex B7) samples.

Examples of microstructure file names: 

"b7d19b.jpg": b7 sample treated at Gleeble corresponding to dilatometric file "SteelB1.D19", second picture 

"b7d21x500a.jpg": b7 sample treated at Gleeble corresponding to dilatometric file "SteelB1.D21", fist picture taken using a magnification of 500x.  
